Laser-cavity locking utilizing beam ellipticity: accessing the 10<sup>7</sup> instability scale relative to cavity linewidth
F.R. Diorico, A. Zhutov, O. Hosten, Optica 11 (2024) 26–31.

Inverse design of spontaneous parametric downconversion for generation of high-dimensional qudits
E. Rozenberg, A. Karnieli, O. Yesharim, J. Foley-Comer, S. Trajtenberg-Mills, D. Freedman, A.M. Bronstein, A. Arie, Optica 9 (2022) 602–615.

Sensitivity limits of millimeter-wave photonic radiometers based on efficient electro-optic upconverters
G. Botello, F. Sedlmeir, A.R. Rueda Sanchez, K. Abdalmalak, E. Brown, G. Leuchs, S. Preu, D. Segovia Vargas, D. Strekalov, L. Munoz, H. Schwefel, Optica 5 (2018) 1210–1219.